{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Power input","Heating","","Nom.","kW","0.03","0.030","0.030"]
["","Cooling","","Nom.","kW","0.03","0.030","0.030"]
["Sound power level","Heating","","","dBA","56","57","59"]
["Control systems","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Fan","Air flow rate","Cooling","High","m³/min","10.7","12.1","15.0"]
["","","Heating","High","m³/min","11.7","13.3","14.4"]
["","","","Low","m³/min","5.3","5.6","6.6"]
["","","Heating","Low","m³/min","6.7","6.9","7.7"]
["Dimensions","Unit","","Width","mm","798","798","798"]
["","","","Height","mm","295","295","295"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.5","8.4","9.2"]
["Dimensions","Unit","","Depth","mm","372","372","372"]
["Sound pressure level","Heating","","Silent operation","dBA","19","19","24"]
["Fan","Air flow rate","Heating","Silent operation","m³/min","4.8","4.8","5.9"]
["","","Cooling","Silent operation","m³/min","4","4.0","4.6"]
["Sound pressure level","Cooling","","High","dBA","38","42","47"]
["Weight","Unit","","","kg","15","15","15"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35"]
["Sound pressure level","Cooling","","Low","dBA","26","27","30"]
["Piping connections","Gas","","OD","mm","9.5","9.5","9.5"]
["Sound pressure level","Cooling","","Silent operation","dBA","19","19","23"]
["Casing","Colour","","","","White","White","White"]
["Sound pressure level","Heating","","Low","dBA","28","29","31"]
["Sound power level","Cooling","","","dBA","54","57","60"]
["Sound pressure level","Heating","","High","dBA","39","42","44"]
["","Cooling","","Nom.","dBA","33","35","38"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.6","9.2","10.7"]
["Sound pressure level","Heating","","Nom.","dBA","35","36","38"]
["Standard Accessories","Wireless remote control","","","","1","1","1"]
["","Photocatalytic air purifying and deodorising filter","","","","1","1","1"]
["","Dry batteries","","","","2","2","2"]
["","Indoor unit fixing screws","","","","3","3","3"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Power supply","Name","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Power supply-=-Voltage","","Voltage","","220-240","220-240","220-240"]
["","Power supply-=-Frequency","","Frequency","","50","50","50"]
["Notes","","","","","(1) - 230V","(1) - Back of heat exchanger","(1) - Back of heat exchanger"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - Front of heat exchanger","(3) - 230V"]
["","","","","","(4) - Back of heat exchanger","(4) - 230V","(4) - Front of heat exchanger"]
["","","","","","(5) - Front of heat exchanger","(5) - 240V","(5) - 240V"]