{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":14,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","","FXFA20A2VEB","FXFA25A2VEB","FXFA32A2VEB","FXFA40A2VEB","FXFA50A2VEB","FXFA63A2VEB","FXFA80A2VEB","FXFA100A2VEB","FXFA125A2VEB"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","9.52","9.52","9.52","12.70","12.70","12.70","12.70","15.90","15.90"]
["","","","OD","mm","6","6","6","6","6","6","6","10","10"]
["Decoration panel 2","Dimensions","","Width","mm","950","950","950","950","950","950","950","950","950"]
["","","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["Piping connections","Gas","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["Decoration panel 2","Dimensions","","Height","mm","148","148","148","148","148","148","148","148","148"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.017","0.017","0.017","0.018","0.023","0.028","0.045","0.078","0.103"]
["Decoration panel 3","Weight","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["","Dimensions","","Height","mm","106","106","106","106","106","106","106","106","106"]
["","","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["Decoration panel","Weight","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Decoration panel 2","Model","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["Decoration panel 3","Model","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Dimensions","","Width","mm","950","950","950","950","950","950","950","950","950"]
["Decoration panel","Dimensions","","Height","mm","65","65","65","65","65","65","65","65","65"]
["Decoration panel 2","Weight","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Decoration panel","Dimensions","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["Sound pressure level","Heating","","At low fan speed","dBA","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["Piping connections","Drain","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Decoration panel","Model","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["Air filter","Type","","","","Resin net","Resin net","Resin net","Resin net","Resin net","Resin net","Resin net","Resin net","Resin net"]
["Decoration panel","Dimensions","","Width","mm","950","950","950","950","950","950","950","950","950"]
["Fan","Air flow rate - 50Hz","Cooling","At low fan speed","m³/min","8.9","8.9","8.9","10.4","10.7","10.7","13.8","13.8","20.6"]
["","","","At high fan speed","m³/min","12.8","12.8","12.8","14.8","15.1","16.6","23.3","28.8","33.0"]
["Power input - 50Hz","Heating","","At high fan speed","kW","0.017","0.017","0.017","0.018","0.023","0.028","0.045","0.078","0.103"]
["Sound pressure level","Cooling","","At low fan speed","dBA","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["","Heating","","At high fan speed","dBA","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["","","","At medium fan speed","dBA","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","At medium fan speed","dBA","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","At high fan speed","dBA","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["Sound power level","Cooling","","At high fan speed","dBA","49.0","49.0","49.0","51.0","51.0","53.0","55.0","60.0","61.0"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","","kg","18","18","18","19","21","21","24","24","26"]
["Dimensions","Unit","","Depth","mm","840","840","840","840","840","840","840","840","840"]
["","","","Width","mm","840","840","840","840","840","840","840","840","840"]
["","","","Height","mm","204","204","204","204","204","204","246","246","288"]
["Heating capacity","Total capacity","","At high fan speed","kW","2.50","3.20","4.00","5.00","6.30","8.00","10.00","12.50","16.00"]
["Cooling capacity","Total capacity","","At high fan speed","kW","2.20","2.80","3.60","4.50","5.60","7.10","9.00","11.20","14.00"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8","8","8","8","8","8","8"]
["","Wire clamp material","","","","7","7","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1","1","1"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","6","6","6","6","6","6"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Power supply-=-Frequency","","Frequency","","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting."]