{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":7,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N9"]
[]
[]
[]
[]
["","","","","","4MXM80N2V1B9","4MXM68N2V1B9"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","49.0"]
["","Refrigeración","","Nom.","dBA","48.0"]
["Accesorios estándar","Manual de instalación","","","","1"]
["","Bolsa de tornillos","","","","1"]
["","Tapón de drenaje","","","","1"]
["","Conjunto reductor","","","","1"]
["","Tapón de drenaje (1)","","","","6"]
["","Tapón de drenaje (2)","","","","3"]
["Refrigerante","Charge","","","TCO2Eq","1.62"]
["","GWP","","","","675.0"]
["","Carga","","","kg","2.40"]
["","Tipo","","","","R-32"]
["Rango de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","46"]
["","","","Mín.","°CBS","-10"]
["Conexiones de tubería","Diferencia de nivel","Ud. int. – Ud. int.","Máx.","m","7.5"]
["","","Ud. int. – Ud. ext.","Máx.","m","15.0"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)"]
["","Longitud de tubería total","Sistema","Real","m","70"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado"]
["Dimensiones","Unidad","","Anchura","mm","974"]
["","","","Profundidad","mm","401"]
["","","","Altura","mm","734"]
["Peso","Unidad","","","kg","67.0"]
["Power supply","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]
["Notas","","","","","(1) - Para una habitación"]
["","","","","","(2) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(3) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","(4) - Contiene gases fluorados de efecto invernadero"]
["Dimensiones","Unidad","","Altura","mm","","734"]
["","","","Anchura","mm","","958"]
["","","","Profundidad","mm","","340"]
["Peso","Unidad","","","kg","","63"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","","420"]
["","","Calefacción","Súper baja","rpm","","420"]
["Compresor","Tipo","","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","-10"]
["","","","Máx.","°CBS","","46"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","","48"]
["","Calefacción","","Nom.","dBA","","49.0"]
["Refrigerante","Tipo","","","","","R-32"]
["","Carga","","","kg","","2"]
["","Carga","","","tCO2Eq","","1.35"]
["","GWP","","","","","675.0"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","25 (1)"]
["","Carga de refrigerante adicional.","","","kg/m","","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","15.0"]
["","","Ud. int. – Ud. int.","Máx.","m","","7.5"]
["","Longitud de tubería total","Sistema","Real","m","","60"]
["Accesorios estándar","Installation manual","","","","","1"]
["","Drain cap (1)","","","","","6"]
["","Drain cap (2)","","","","","3"]
["","Drain plug","","","","","1"]
["","Reducer assembly","","","","","1"]
["","Screw bag","","","","","1"]
["Alimentación eléctrica","Fase","","","","","1~"]
["","Frecuencia","","","Hz","","50"]
["","Tensión","","","V","","220-240"]
["Notas","","","","","","(1) - Para una habitación"]