{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":11,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA125A2VEB","ADEA35A2VEB","ADEA60A2VEB","ADEA50A2VEB","ADEA71A2VEB","ADEA100A2VEB"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","38","37","31"]
["","","","Medio","dBA","35","34","28"]
["","","","Bajo","dBA","32","29","25"]
["","Refrigeración","","Medio","dBA","35","32","28"]
["","","","Bajo","dBA","32","29","25"]
["","","","Alto","dBA","37","35","30"]
["Accesorios estándar","Manual de uso","","","","1","1","1","","1"]
["","Manual de instalación","","","","1","1","1","","1"]
["","Tubo flexible de drenaje","","","","1","1","1","","1"]
["","Abrazadera metálica para el tubo de drenaje","","","","1","1","1","","1"]
["","Arandela para ménsula de suspensión","","","","8","8","8","","8"]
["","Tornillos","","","","40","40","40","","40"]
["","Aislamiento para adaptador","","","","2","2","2","","2"]
["","Almohadillas de sellado","","","","5","5","5","","5"]
["","Abrazaderas","","","","4","4","4","","4"]
["Sistemas de control","Controlador remoto con cable","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","14.00"]
["Conexiones de tubería","Liquid","","OD","mm","9.52","6.35","6.35"]
["","Gas","","D.E.","mm","15.90","9.52","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","62","60","56"]
["Dimensiones","Unidad","","Anchura","mm","1,400","700","1,000"]
["","","","Profundidad","mm","800","800","800"]
["","","","Altura","mm","245","245","245"]
["Carcasa","Material","","","","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado"]
["","Color","","","","No pintada (galvanizada)","No pintada (galvanizada)","No pintada (galvanizada)"]
["Peso","Unidad","","","kg","46.0","28.0","35.0"]
["Ventilador","Presión estática externa","","Alto","Pa","150","150","150"]
["","","","Nom.","Pa","50","30","30"]
["Altura de drenaje","mm","","","","625","625","625"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","13.50"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","220-240/220","220-240/220","220-240/220"]
["Notas","","","","","(1) - El nivel de potencia sonora es un valor absoluto que genera una fuente de sonido.","(1) - El nivel de potencia sonora es un valor absoluto que genera una fuente de sonido.","(1) - El nivel de potencia sonora es un valor absoluto que genera una fuente de sonido.","","(1) - El nivel de potencia sonora es un valor absoluto que genera una fuente de sonido."]
["","","","","","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","","(2) - Consulte en el plano independiente con los datos eléctricos."]
["Accesorios estándar","AAA dry-cell batteries","","","","","","","3"]
["Ventilador","Presión estática externa","","Alto","Pa","","","","","150","150"]
["Carcasa","Color","","","","","","","","No pintada (galvanizada)"]
["","Material","","","","","","","","Placa de acero galvanizado","Placa de acero galvanizado"]
["Dimensiones","Unidad","","Altura","mm","","","","","245","245"]
["","","","Anchura","mm","","","","","1000","1400"]
["","","","Profundidad","mm","","","","","800","800"]
["Peso","Unidad","","","kg","","","","","35"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","","","","18","29"]
["","","","Medio","m³/min","","","","","15"]
["","","","Bajo","m³/min","","","","","12.5","23"]
["","","Calefacción","Alto","m³/min","","","","","18","29"]
["","","","Medio","m³/min","","","","","15"]
["","","","Bajo","m³/min","","","","","12.5","23"]
["","Presión estática externa","","Nom.","Pa","","","","","30","40"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","","56","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","","","30","34"]
["","","","Medio","dBA","","","","","28"]
["","","","Bajo","dBA","","","","","25","30"]
["","Calefacción","","Alto","dBA","","","","","31","36"]
["","","","Medio","dBA","","","","","28","33"]
["","","","Bajo","dBA","","","","","25","30"]
["Conexiones de tubería","Líquido","","D.E.","mm","","","","","9.52","9.52"]
["","Gas","","D.E.","mm","","","","","15.9"]
["","Drenaje","","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Altura de drenaje","mm","","","","","","","","625","625"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","","","","","BRC4C65, BRC4C66"]
["","Controlador remoto con cable","","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Alimentación eléctrica","Fase","","","","","","","","1~","1~"]
["","Frecuencia","","","Hz","","","","","50","50"]
["","Tensión","","","V","","","","","220-240/220","220-240/220"]
["Carcasa","Color","","","","","","","","","No pintada (galvanizada)"]
["Peso","Unidad","","","kg","","","","","","46"]
["Ventilador","Caudal de aire","Refrigeración","Medio","m³/min","","","","","","26"]
["","","Calefacción","Medio","m³/min","","","","","","26"]
["Nivel de presión sonora","Refrigeración","","Medio","dBA","","","","","","32"]
["Conexiones de tubería","Gas","","D.E.","mm","","","","","","15.9"]
["Sistemas de control","Infrared remote control","","","","","","","","","BRC4C65, BRC4C66"]
["","Controlador remoto con cable","","","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accesorios estándar","Installation manual","","","","","","","","","1"]
["","Washer for hanger bracket","","","","","","","","","8"]
["","Operation manual","","","","","","","","","1"]
["","Clamps","","","","","","","","","4"]
["","Drain hose","","","","","","","","","1"]
["","Insulation for fitting","","","","","","","","","2"]
["","Metal clamp for drain hose","","","","","","","","","1"]
["","Screws","","","","","","","","","40"]
["","Sealing pads","","","","","","","","","5"]