{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-J3"]
[]
[]
[]
[]
["","","","","","ATX25J3V1B","ATX35J3V1B","ATX20J3V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","40","41","39"]
["","","","Medio","dBA","34","35","34"]
["","","","Funcionamiento silencioso","dBA","25","26","25"]
["","","","Bajo","dBA","28","29","28"]
["","Refrigeración","","Medio","dBA","33","34","33"]
["","","","Funcionamiento silencioso","dBA","22","23","22"]
["","","","Bajo","dBA","26","27","25"]
["","","","Alto","dBA","40","41","39"]
["Accesorios estándar","Manual de instalación","","","","1","1","1"]
["","Manual de uso","","","","1","1","1"]
["","Mando a distancia sin cable","","","","1","1","1"]
["","Pilas secas AAA","","","","2","2","2"]
["","Soporte del mando a distancia","","","","1","1","1"]
["","Placa de montaje","","","","1","1","1"]
["","Filtro desodorizante de apatito de titanio","","","","2","2","2"]
["","Tornillos de fijación de la unidad interior","","","","2","2","2"]
["Sistemas de control","Infrared remote control","","","","ARC433A89","ARC433A89","ARC433A89"]
["Conexiones de tubería","Liquid","","OD","mm","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.50","9.50","9.50"]
["","Drain","","","","18","18","18"]
["Consumo","Refrigeración","","Nom.","kW","0.030","0.030","0.030"]
["","Calefacción","","Nom.","kW","0.040","0.040","0.040"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55.0","58","55"]
["","Calefacción","","","dBA","55","58","55"]
["Dimensiones","Unidad","","Anchura","mm","770","770","770"]
["","","","Profundidad","mm","283","283","283"]
["","","","Altura","mm","198","198","198"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco"]
["Peso","Unidad","","","kg","7.00","7.00","7.00"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","","9.4"]
["","","","Bajo","m³/min","","","6.3"]
["","","","Medio","m³/min","","","7.8"]
["","","","Funcionamiento silencioso","m³/min","","","5.5"]
["","","Refrigeración","Bajo","m³/min","","","5.9"]
["","","","Medio","m³/min","","","7.4"]
["","","","Alto","m³/min","","","9.1"]
["","","","Funcionamiento silencioso","m³/min","","","4.7"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Nombre","","","","V1","V1","V1"]
["","Tensión","","","V","220-240","220-240","220-240"]
["Notas","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 5m; diferencia de nivel 0m","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 5m; diferencia de nivel 0m","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 5m; diferencia de nivel 0m"]
["","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m; diferencia de nivel 0m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m; diferencia de nivel 0m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m; diferencia de nivel 0m"]