{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K2V1B","ATX35K5V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","39","39","40","40","43","43"]
["","","Medio","dBA","34","34","34","34","35","35"]
["","","Funcionamiento silencioso","dBA","23","23","23","23","26","26"]
["","","Bajo","dBA","28","28","28","28","29","29"]
["","Refrigeración","Medio","dBA","33","33","33","33","34","34"]
["","","Funcionamiento silencioso","dBA","20","20","20","20","20","20"]
["","","Bajo","dBA","25","25","26","26","27","27"]
["","","Alto","dBA","39","39","40","40","43","43"]
["Accesorios estándar","Manual de instalación","","","1","1","1","1","1","1"]
["","Manual de uso","","","1","1","1","1","1","1"]
["","Mando a distancia por infrarrojos","","","1","1","1","1","1","1"]
["","Pilas secas AA","","","2","","2","","2"]
["","Soporte del mando a distancia","","","1","1","1","1","1","1"]
["","Placa de montaje","","","1","1","1","1","1","1"]
["","Filtro desodorizante de apatito de titanio","","","2","2","","2","","2"]
["","Tornillos de fijación de la unidad interior","","","2","2","2","2","2","2"]
["Sistemas de control","Controlador remoto con cable","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.50","9.50","9.50","9.50","9.50","9.50"]
["","Drain","","","18","18","18","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.018","0.018","0.020","0.020","0.024","0.024"]
["","Calefacción","Nom.","kW","0.022","0.022","0.023","0.023","0.029","0.029"]
["Nivel de potencia sonora","Refrigeración","","dBA","55","55","55","55","58","58"]
["","Calefacción","","dBA","55","55","55","55","58","58"]
["Dimensiones","Unidad","Anchura","mm","770","770","770","770","770","770"]
["","","Profundidad","mm","225","225","225","225","225","225"]
["","","Altura","mm","286","286","286","286","286","286"]
["Carcasa","Color","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","8.5","8.5","8.5","8.5","9.0","9.0"]
["Power supply","Fase","","","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50","50","50"]
["","Nombre","","","V1","V1","V1","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire.","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire.","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire."]
["Accesorios estándar","Pilas secas AAA","","","","2","","2","","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","","","2","","2"]