{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M"]
[]
[]
[]
[]
["","","","","ATXM20M2V1B","ATXM25M2V1B","ATXM35M2V1B","ATXM50M2V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","39","39","39","43"]
["","","Medio","dBA","34","34","35","39"]
["","","Funcionamiento silencioso","dBA","20","20","20","31"]
["","","Bajo","dBA","26","27","28","34"]
["","Refrigeración","Medio","dBA","33","33","33","40"]
["","","Funcionamiento silencioso","dBA","19","19","19","32"]
["","","Bajo","dBA","25","25","29","36"]
["","","Alto","dBA","41","41","45","44"]
["Accesorios estándar","Manual de instalación","","","1","1","1","1"]
["","Manual de uso","","","1","1","1","1"]
["","Mando a distancia sin cable","","","1","1","1","1"]
["","Pilas secas AAA","","","2","2","2","2"]
["","Soporte del mando a distancia","","","1","1","1","1"]
["","Placa de montaje","","","1","1","1","1"]
["","Filtro desodorizante de apatito de titanio","","","1","1","1","2"]
["","Tornillos de fijación de la unidad interior","","","2","2","2","2"]
["Sistemas de control","Controlador remoto con cable","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073"]
["","Infrared remote control","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.50","9.50","9.50","12.7"]
["","Drain","","","18","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.030","0.030","0.035","0.030"]
["","Calefacción","Nom.","kW","0.025","0.025","0.025","0.032"]
["Nivel de potencia sonora","Refrigeración","","dBA","58","58","60","59"]
["","Calefacción","","dBA","55","55","55","58"]
["Dimensiones","Unidad","Anchura","mm","811","811","811","1,040"]
["","","Profundidad","mm","272","272","272","295"]
["","","Altura","mm","294","294","294","300"]
["Carcasa","Color","","","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","10.0","10.0","10.0","14.5"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50"]
["","Nombre","","","V1","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240","220-240"]