{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","38","38","41","41"]
["","","Medio","dBA","","33","","36"]
["","","Funcionamiento silencioso","dBA","21","21","21","21"]
["","","Bajo","dBA","28","28","30","30"]
["","Refrigeración","Medio","dBA","","31","","35"]
["","","Funcionamiento silencioso","dBA","21","21","21","21"]
["","","Bajo","dBA","25","25","28","28"]
["","","Alto","dBA","37","37","42","42"]
["","","Nom.","dBA","33"]
["","Refrigeración","Nom.","dBA","31","","35"]
["Accesorios estándar","Manual de instalación","","","1","1","1","1"]
["","Manual de uso","","","1","1","1","1"]
["","Mando a distancia sin cable","","","1","1","1","1"]
["","Pilas","","","2","","2"]
["","Soporte del mando a distancia","","","1","1","1","1"]
["","Placa de montaje","","","1","1","1","1"]
["","Tornillos de fijación de la unidad interior","","","2","2","2","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","2","","2"]
["Sistemas de control","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A6","ARC466A6"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.5","9.50","9.5","9.50"]
["","Drain","","","18","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.040","0.040","0.040","0.040"]
["","Calefacción","Nom.","kW","0.040","0.040","0.040","0.040"]
["Nivel de potencia sonora","Refrigeración","","dBA","55","55","59","59"]
["","Calefacción","","dBA","56","56","58","58"]
["Dimensiones","Unidad","Anchura","mm","780","780","780","780"]
["","","Profundidad","mm","215","215","215","215"]
["","","Altura","mm","289","289","289","289"]
["Carcasa","Color","","","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","8","8.00","8","8.00"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50"]
["","Nombre","","","V1","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240","220-240"]
["Notas","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Accesorios estándar","Pilas secas AAA","","","","2","","2"]
["","Filtro desodorizante de apatito de titanio","","","","2","","2"]
["Notas","","","","","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar."]