{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A1A"]
[]
[]
[]
[]
["","","","","","D2CND024A1AA","D2CND024A1AB","D2CND028A1AA","D2CND028A1AB","D2CND035A1AA","D2CND035A1AB"]
["Pérdidas de calor","Caldera de reserva Ps","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Agua caliente sanitaria","Consumo térmico (valor calorífico bruto) Qnw","Nom.","Máx.","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","","","Mín.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","Consumo térmico (valor calorífico neto) Qnw","Nom.","Mín.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Máx.","kW","23.5","23.5","29.5","29.5","34","34"]
["Gas de combustión","Flujo de masa (G31)","","Máx.","kg/h","36.0","36","43.3","43.3","54.7","54.7"]
["Supply air","Concentric","","","","Sí","Sí","Sí","Sí","Sí","Sí"]
["Calentamiento de agua caliente sanitaria","General","","Clase de eficiencia energética para calentamiento de agua","","A","A","A","A","A","A"]
["","","","Perfil de carga declarado","","XL","XL","XL","XL","XL","XL"]
["Dimensiones","Unidad","Altura","Carcasa","mm","590","590","690","690","690","690"]
["Carcasa","Material","","","","Metal laminado","Metal laminado","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo"]
["","Color","","","","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)"]
["Calef. de habitaciones","General","","Clase de eficiencia de calefacción de espacios estacional","","A","A","A","A","A","A"]
["Calefacción central","Consumo térmico Qn (valor calorífico bruto)","Nom.","Mín.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Máx.","kW","26.1","26.1","30","30","37.8","37.8"]
["","Eficiencia","","Net calorific value","%","97.9","97.9"]
["","","","Valor calorífico bruto","%","87.3","87.3"]
["","Consumo térmico Qn (valor calorífico neto)","Nom.","Máx.","kW","23.5","23.5","27","27","34","34"]
["","","","Mín.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["Gas","Clase NOx","","","","6","6","6","6","6","6"]