{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2TND-A4A"]
[]
[]
[]
[]
["","","","","","D2TND012A4AA","D2TND012A4AB","D2TND018A4AA","D2TND018A4AB","D2TND024A4AA","D2TND024A4AB","D2TND028A4AA","D2TND028A4AB","D2TND035A4AA","D2TND035A4AB"]
["Pérdidas de calor","Caldera de reserva Ps","","","kW","0.057","0.057","0.057","0.057","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Agua caliente sanitaria","Consumo térmico (valor calorífico bruto) Qnw","Nom.","Máx.","kW","12.4","12.3","18.1","18.1","26.1","26.1","32.7","32.7","37.7","37.7"]
["","","","Mín.","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3","5.3","5.3"]
["","Temperatura","","Máx.","°C","60","","60","","60","","60","","60"]
["","Consumo térmico (valor calorífico neto) Qnw","Nom.","Mín.","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Máx.","kW","11.2","11.1","17.0","16.9","23.5","25.3","29.5","29.5","34","34"]
["Gas de combustión","Temperatura","","Máx.","°C","90","","90","","90","","76.4","","81.7"]
["","Flujo de masa (G31)","","Máx.","kg/h","36.0","36","36.0","36","36.0","36","43.3","43.3","54.7","54.7"]
["Supply air","Concentric","","","","Sí","Sí","Sí","Sí","Sí","Sí","Sí","Sí","Sí","Sí"]
["Dimensiones","Unidad","Altura","Carcasa","mm","590","590","590","590","590","590","690","690","690","690"]
["Carcasa","Material","","","","Metal laminado","Metal laminado","Metal laminado","Metal laminado","Metal laminado","Metal laminado","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo","Chapa de acero galvanizado pintada al polvo"]
["","Color","","","","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)","Blanco titanio (RAL9003)"]
["Calef. de habitaciones","General","","Clase de eficiencia de calefacción de espacios estacional","","A","A","A","A","A","A","A","A","A","A"]
["","","","ηs (eficiencia de calefacción de espacios estacional)","%","93","","93","","93","","93","","93"]
["Calefacción central","Consumo térmico Qn (valor calorífico bruto)","Nom.","Mín.","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Máx.","kW","12.4","12.3","18.9","18.8","26.1","26.1","30","30","37.8","37.8"]
["","Eficiencia","","Net calorific value","%","98.6","98.6","98.2","98.18","97.9","97.9"]
["","","","Valor calorífico bruto","%","87.8","87.8","87.4","87.4","87.3","87.3"]
["","Temperatura del agua","","Máx.","°C","100","","100","","100","","100","","100"]
["","Potencia Pn a 80/60°C","","Mín.","kW","2.8","","2.8","","2.8","","4.6","","4.6"]
["","","","Nom.","kW","10.9","","16.6","","22.8","","26.3","","33.2"]
["","Consumo térmico Qn (valor calorífico neto)","Nom.","Máx.","kW","11.2","11.1","17.0","16.9","23.5","23.5","27","27","34","34"]
["","","","Mín.","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8","4.8","4.8"]
["","Potencia Pnb a 50/30°C","","Mín.","kW","3.1","","3.1","","3.1","","5.2","","5.2"]
["","","","Nom.","kW","12.0","","18.0","","24.0","","28.2","","35"]
["Gas","Consumo (G31)","","Mín.","m³/h","0.12","","0.12","","0.12","","0.2","","0.2"]
["","","","Máx.","m³/h","0.46","","0.69","","0.96","","1.1","","1.38"]
["","Clase NOx","","","","6","6","6","6","6","6","6","6","6","6"]