{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Temperatura ambiente","Humedad relativa <","","","%","85"]
["Número máximo de unidades interiores conectables","","","","","32"]
["Consumo","kW","","","","0.015 (1)"]
["Comunicación","DIII-NET","","Cantidad","","1"]
["","","","Observación","","DIII-NET (F1F2)"]
["","Ethernet","","Cantidad","","1"]
["","Terminal de entrada","Digital","Cantidad","","4"]
["Dimensiones","Unidad","","Anchura","mm","384"]
["","","","Profundidad","mm","92"]
["","","","Altura","mm","136"]
["Número máximo de unidades exteriores conectables","","","","","7"]
["Power supply","Frecuencia","","","Hz","50/60"]
["","Tensión","","","V","110-240 CA"]
["Notas","","","","","(1) - Incluye la entrada de alimentación para la interfaz WAGO, el módulo CPU, el módulo de E/S"]
["","","","","","(2) - Las dimensiones incluyen el suministro de alimentación de la interfaz WAGO, el módulo CPU, el módulo de E/S y todo el espacio necesario entre los distintos componentes"]
["","","","","","(3) - Las dimensiones de la pantalla opcional son: altura: 209 mm, anchura: 123 mm, profundidad: 8,5 mm"]