{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA50A2VEB9","FFA60A2VEB9"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","31.0","34.0","39.0","43.0"]
["","","","Medio","dBA","28.5","30.5","34.0","40.0"]
["","","","Bajo","dBA","25.0","25.0","27.0","32.0"]
["","Refrigeración","","Medio","dBA","28.5","30.5","34.0","40.0"]
["","","","Bajo","dBA","25.0","25.0","27.0","32.0"]
["","","","Alto","dBA","31.0","34.0","39.0","43.0"]
["Accesorios estándar","Manual de instalación y de uso","","","","1","1","1","1"]
["","Tubo flexible de drenaje","","","","1","1","1","1"]
["","Abrazadera de tubo flexible","","","","1","1","1","1"]
["","Arandela para ménsula de suspensión","","","","8","8","8","8"]
["","Tornillos","","","","4","4","4","4"]
["","Tubo de aislamiento térmico","","","","2","2","2","2"]
["","Material de sellado","","","","4","4","4","4"]
["","Arrollamientos de unión","","","","7","7","7","7"]
["Sistemas de control","Controlador remoto con cable","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)"]
["Conexiones de tubería","Liquid","","OD","mm","6","6","6","6"]
["","Gas","","D.E.","mm","9.52","9.52","12.70","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Panel decorativo 4","Dimensiones","","Profundidad","mm","700","700","700","700"]
["","","","Anchura","mm","700","700","700","700"]
["","","","Altura","mm","55","55","55","55"]
["","Modelo","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Color","","","","BLANCO (RAL9010)","BLANCO (RAL9010)","BLANCO (RAL9010)","BLANCO (RAL9010)"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Nivel de potencia sonora","Refrigeración","","","dBA","48.0","51.0","56.0","60.0"]
["Dimensiones","Unidad","","Anchura","mm","575","575","575","575"]
["","","","Profundidad","mm","575","575","575","575"]
["","","","Altura","mm","260","260","260","260"]
["Carcasa","Material","","","","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado"]
["Peso","Unidad","","","kg","16.0","16.0","17.5","17.5"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","9.0","10.0","12.7","14.5"]
["","","","Bajo","m³/min","6.5","6.5","8.6","9.5"]
["","","","Medio","m³/min","8.0","8.5","10.9","12.5"]
["","","Refrigeración","Bajo","m³/min","6.5","6.5","8.6","9.5"]
["","","","Medio","m³/min","8.0","8.5","10.9","12.5"]
["","","","Alto","m³/min","9.0","10.0","12.7","14.5"]
["Panel decorativo","Peso","","","kg","2.8","2.8","2.8","2.8"]
["","Modelo","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Dimensiones","","Altura","mm","46","46","46","46"]
["","","","Profundidad","mm","620","620","620","620"]
["","","","Anchura","mm","620","620","620","620"]
["","Color","","","","Blanco (N9.5)","Blanco (N9.5)","Blanco (N9.5)","Blanco (N9.5)"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240"]