{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":93,"n_cols":12,"rows_kept":93,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM20M2V1B","FTXM25M2V1B","FTXM35M2V1B","FTXM50M2V1B","FTXM60M2V1B","FTXM71M2V1B","FTXM42M2V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","39","39","39","43","45","46"]
["","","","Medio","dBA","34","34","35","39","41","42"]
["","","","Funcionamiento silencioso","dBA","20","20","20","31","33","34"]
["","","","Bajo","dBA","26","27","28","34","36","37"]
["","Refrigeración","","Medio","dBA","33","33","33","40","42","43"]
["","","","Funcionamiento silencioso","dBA","19","19","19","32","34","35"]
["","","","Bajo","dBA","25","25","29","36","37","38"]
["","","","Alto","dBA","41","41","45","44","46","47"]
["Accesorios estándar","Manual de instalación","","","","1","1","1","1","1","1"]
["","Manual de uso","","","","1","1","1","1","1","1"]
["","Mando a distancia sin cable","","","","1","1","1","1","1","1"]
["","Pilas secas AAA","","","","2","2","2","2","2","2"]
["","Soporte del mando a distancia","","","","1","1","1","1","1","1"]
["","Placa de montaje","","","","1","1","1","1","1","1"]
["","Filtro desodorizante de apatito de titanio","","","","1","1","1","2","2","2"]
["","Tornillos de fijación de la unidad interior","","","","2","2","2","2","2","2"]
["Sistemas de control","Controlador remoto con cable","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073"]
["","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Conexiones de tubería","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.50","9.50","9.50","12.7","12.7","15.90"]
["","Drain","","","","18","18","18","18","18","18"]
["Consumo","Refrigeración","","Nom.","kW","0.030","0.030","0.035","0.030","0.032","0.054"]
["","Calefacción","","Nom.","kW","0.025","0.025","0.025","0.032","0.035","0.060"]
["Nivel de potencia sonora","Refrigeración","","","dBA","57","57","60","59","60","60"]
["","Calefacción","","","dBA","54","54","54","58","59","61"]
["Dimensiones","Unidad","","Anchura","mm","811","811","811","1,040","1,040","1,040"]
["","","","Profundidad","mm","272","272","272","295","295","295"]
["","","","Altura","mm","294","294","294","300","300","300"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","","kg","10.0","10.0","10.0","14.5","14.5","14.5"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","10.4","10.4","10.4","17.1"]
["","","","Bajo","m³/min","6.5","6.8","7.1","12.2"]
["","","","Medio","m³/min","8.7","8.7","9.0","14.6"]
["","","","Funcionamiento silencioso","m³/min","5.3","5.3","5.3","10.7"]
["","","Refrigeración","Bajo","m³/min","6.0","6.2","6.4","11.6"]
["","","","Medio","m³/min","7.9","8.1","8.3","14.2"]
["","","","Alto","m³/min","11.1","11.1","12.6","16.5"]
["","","","Funcionamiento silencioso","m³/min","4.4","4.4","4.6","10.3"]
["Power supply","Fase","","","","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50"]
["","Nombre","","","","V1","V1","V1","V1","V1","V1"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero"]
["","","","","","","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5 m"]
["","","","","","","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m"]
["Consumo","Refrigeración","","Nom.","kW","","","","","","","0.035"]
["","Calefacción","","Nom.","kW","","","","","","","0.035"]
["Carcasa","Color","","","","","","","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","","","","","","","294"]
["","","","Anchura","mm","","","","","","","811"]
["","","","Profundidad","mm","","","","","","","272"]
["Peso","Unidad","","","kg","","","","","","","10"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","","","","","","12.6"]
["Ventilador","Caudal de aire","Refrigeración","Medio","m³/min","","","","","","","9.5"]
["Ventilador","Caudal de aire","Refrigeración","Bajo","m³/min","","","","","","","7.1"]
["","","","Funcionamiento silencioso","m³/min","","","","","","","4.6"]
["","","Calefacción","Alto","m³/min","","","","","","","13"]
["Ventilador","Caudal de aire","Calefacción","Medio","m³/min","","","","","","","10.4"]
["Ventilador","Caudal de aire","Calefacción","Bajo","m³/min","","","","","","","7.1"]
["","","","Funcionamiento silencioso","m³/min","","","","","","","5.3"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","","","","60"]
["","Calefacción","","","dBA","","","","","","","60"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","","","","","45"]
["Nivel de presión sonora","Refrigeración","","Medio","dBA","","","","","","","39"]
["Nivel de presión sonora","Refrigeración","","Bajo","dBA","","","","","","","30"]
["","","","Funcionamiento silencioso","dBA","","","","","","","21"]
["","Calefacción","","Alto","dBA","","","","","","","45"]
["","","","Medio","dBA","","","","","","","39"]
["","","","Bajo","dBA","","","","","","","29"]
["","","","Funcionamiento silencioso","dBA","","","","","","","21"]
["Conexiones de tubería","Líquido","","D.E.","mm","","","","","","","6.35"]
["Conexiones de tubería","Gas","","D.E.","mm","","","","","","","12.7"]
["Conexiones de tubería","Drenaje","","","","","","","","","","18"]
["Sistemas de control","Infrared remote control","","","","","","","","","","ARC466A33"]
["","Controlador remoto con cable","","","","","","","","","","BRC944B2, BRC073A1"]
["Accesorios estándar","Installation manual","","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","","","","2"]
["","Operation manual","","","","","","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","","1"]
["Alimentación eléctrica","Nombre","","","","","","","","","","V1"]
["","Fase","","","","","","","","","","1~"]
["","Alimentación eléctrica-=-Frecuencia","","Frecuencia","","","","","","","","50"]
["","Alimentación eléctrica-=-Tensión","","Tensión","","","","","","","","220-240"]