{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":14,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B","FTXS25K3V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","40","40","41","45","45","45","45","47","47","41"]
["","","Medio","dBA","","34","","","39","","39","","40","34"]
["","","Funcionamiento silencioso","dBA","19","19","19","19","19","22","22","24","24","19"]
["","","Bajo","dBA","27","27","27","29","29","33","33","34","34","27"]
["","Refrigeración","Medio","dBA","","32","","","37","","39","","40","33"]
["","","Funcionamiento silencioso","dBA","19","19","19","19","19","21","21","23","23","19"]
["","","Bajo","dBA","24","24","25","29","29","33","33","34","34","25"]
["","","Alto","dBA","40","40","41","45","45","45","45","46","46","41"]
["","","Nom.","dBA","34","","34","39","","39","","40"]
["","Refrigeración","Nom.","dBA","32","","33","37","","39","","40"]
["Accesorios estándar","Manual de instalación","","","1","1","1","1","1","1","1","1","1","1"]
["","Manual de uso","","","1","1","1","1","1","1","1","1","1","1"]
["","Mando a distancia sin cable","","","1","1","1","1","1","1","1","1","1","1"]
["","Pilas","","","2","","2","2","","2","","2"]
["","Soporte del mando a distancia","","","1","1","1","1","1","1","1","1","1","1"]
["","Placa de montaje","","","1","1","1","1","1","1","1","1","1","1"]
["","Tornillos de fijación de la unidad interior","","","2","2","2","2","2","2","2","2","2","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","2","","2","2","","2","","2"]
["Sistemas de control","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A6","ARC466A6","ARC466A9","ARC466A6","ARC466A9","ARC466A6","ARC466A9","ARC466A6"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.5","9.50","9.5","9.5","9.50","9.5","9.50","12.7","12.7","9.50"]
["","Drain","","","18","18","18","18","18","18","18","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.04","0.040 (1), 0.040 (2), 0.040 (3)","0.04","0.026 (2), 0.026 (3), 0.026 (4)","0.026 (1), 0.026 (2), 0.026 (3)","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (1), 0.024 (2), 0.024 (3)","0.026 (2), 0.026 (3), 0.026 (4)","0.026 (1), 0.026 (2), 0.026 (3)","0.040 (1), 0.040 (2), 0.040 (3)"]
["","Calefacción","Nom.","kW","0.04","0.040 (1), 0.040 (2), 0.040 (3)","0.04","0.028 (2), 0.028 (3), 0.028 (4)","0.028 (1), 0.028 (2), 0.028 (3)","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (1), 0.030 (2), 0.030 (3)","0.032 (2), 0.032 (3), 0.032 (4)","0.032 (1), 0.032 (2), 0.032 (3)","0.040 (1), 0.040 (2), 0.040 (3)"]
["Nivel de potencia sonora","Refrigeración","","dBA","58","58","58","59","59","59","59","60","60","58"]
["","Calefacción","","dBA","58","58","58","59","59","59","59","60","60","58"]
["Dimensiones","Unidad","Anchura","mm","780","780","780","900","900","900","900","900","900","780"]
["","","Profundidad","mm","215","289","215","215","298","215","298","215","298","289"]
["","","Altura","mm","289","215","289","298","215","298","215","298","215","215"]
["Carcasa","Color","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","8","8.00","8","11","11.0","11","11.0","11","11.0","8.00"]
["Power supply","Fase","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Nombre","","","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(1) - 220 V","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(1) - 220 V","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(1) - 220 V","(1) - 220 V"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220 V","(2) - 230V","(2) - 220 V","(2) - 230V","(2) - 220 V","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V"]
["Accesorios estándar","Pilas secas AAA","","","","2","","","2","","2","","2","2"]
["","Filtro desodorizante de apatito de titanio","","","","2","","","2","","2","","2","2"]
["Notas","","","","","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","","(4) - 240V","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(4) - 240V","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(4) - 240V","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar."]