{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA100AVEB9","FUA100AVEB","FUA125AVEB9","FUA125AVEB","FUA71AVEB9","FUA71AVEB"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","46","46","47","47","41","41"]
["","","","Medio","dBA","42","42","43","43","38","38"]
["","","","Bajo","dBA","39","39","40","40","35","35"]
["","Refrigeración","","Medio","dBA","42","42","43","43","38","38"]
["","","","Bajo","dBA","39","39","40","40","35","35"]
["","","","Alto","dBA","46","46","47","47","41","41"]
["Accesorios estándar","Manual de uso","","","","1","1","1","1","1","1"]
["","Manual de instalación","","","","1","1","1","1","1","1"]
["","Tubo flexible de drenaje","","","","1","1","1","1","1","1"]
["","Tubo de aislamiento térmico","","","","3","3","3","3","3","3"]
["","Arrollamientos de unión","","","","10","10","10","10","10","10"]
["","Abrazadera de tubo flexible","","","","1","1","1","1","1","1"]
["","Material de sellado","","","","4","4","4","4","4","4"]
["","Arandela para placa de fijación","","","","1","1","1","1","1","1"]
["","Junta de drenaje","","","","1","1","1","1","1","1"]
["","Tela no tejida","","","","1","1","1","1","1","1"]
["","Arandela","","","","8","8","8","8","8","8"]
["","Tornillo de fijación del tubo de drenaje","","","","5","5","5","5","5","5"]
["Sistemas de control","Controlador remoto con cable","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","","","12.10","12.1"]
["Conexiones de tubería","Liquid","","OD","mm","9.52","9.52","9.52","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Drain","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","64","65","65","","59"]
["","Calefacción","","","dBA","","64","","","","59"]
["Dimensiones","Unidad","","Anchura","mm","950","950","950","950","950","950"]
["","","","Profundidad","mm","950","950","950","950","950","950"]
["","","","Altura","mm","198","198","198","198","198","198"]
["Carcasa","Material","","","","Resina","Resina","Resina","Resina","Resina","Resina"]
["","Color","","","","Blanco fresco","Blanco fresco","Blanco fresco","Blanco fresco","Blanco fresco","Blanco fresco"]
["Peso","Unidad","","","kg","26.0","26.0","26.0","26","25.0","25.0"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","31.0","","32.5","","23.0"]
["","","","Bajo","m³/min","","20.0","","20.5","","16.0"]
["","","","Medio","m³/min","","25.5","","26.5","","19.5"]
["","","Refrigeración","Bajo","m³/min","","20.0","","20.5","","16.0"]
["","","","Medio","m³/min","","25.5","","26.5","","19.5"]
["","","","Alto","m³/min","","31.0","","32.5","","23.0"]
["Altura de drenaje","mm","","","","600","600","600","600","600","600"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","","","13.5","13.5"]