{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB","FVA71AMVEB"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","50","51","53","43"]
["","","","Nom.","dBA","47","48","51","41"]
["","","","Medio","dBA","44","46","48","38"]
["","Refrigeración","","Medio","dBA","47","48","51","41"]
["","","","Bajo","dBA","44","46","48","38"]
["","","","Alto","dBA","50","51","53","43"]
["Accesorios estándar","Tornillos","","","","5","5","5","5"]
["","Manual de instalación","","","","1","1","1","1"]
["","Manual de uso","","","","1","1","1","1"]
["","Casquillo","","","","1","1","1","1"]
["","Arrollamientos de unión","","","","5","5","5","5"]
["","Aislamiento para adaptador de tubos de gas","","","","1","1","1","1"]
["","Aislamiento para adaptador de tubos de líquido","","","","1","1","1","1"]
["","Material a prueba de rocío","","","","1","1","1","1"]
["","Cableado del mando a distancia","","","","1","1","1","1"]
["","Soporte para instalación","","","","1","1","1","1"]
["","Goma de protección de orificios","","","","2","2","2","2"]
["","Cubierta","","","","1","1","1","1"]
["","Patrón de instalación","","","","1","1","1","1"]
["Sistemas de control","Controlador remoto con cable","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","","12.10","13.40"]
["Conexiones de tubería","Liquid","","OD","mm","9.52","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Nivel de potencia sonora","Refrigeración","","","dBA","62","63","65","55"]
["Dimensiones","Unidad","","Anchura","mm","600","600","600","600"]
["","","","Profundidad","mm","350","350","350","270"]
["","","","Altura","mm","1,850","1,850","1,850","1,850"]
["Carcasa","Color","","","","Blanco fresco","Blanco fresco","Blanco fresco","Blanco fresco"]
["Peso","Unidad","","","kg","50","50","50","42"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","28","28","30","18"]
["","","","Bajo","m³/min","22","24","26","14"]
["","","","Medio","m³/min","25","26","28","16"]
["","","Refrigeración","Bajo","m³/min","22","24","26","14"]
["","","","Medio","m³/min","25","26","28","16"]
["","","","Alto","m³/min","28","28","30","18"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","","13.5","15.5"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50/60","50/60","50/60","50/60"]
["","Tensión","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notas","","","","","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos."]