{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":8,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG25K2V1B","FVXG50K2V1B","FVXG35K2V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","39","46"]
["","","","Medio","dBA","32","40"]
["","","","Funcionamiento silencioso","dBA","22","30"]
["","","","Bajo","dBA","26","34"]
["","Refrigeración","","Medio","dBA","32","40"]
["","","","Funcionamiento silencioso","dBA","23","32"]
["","","","Bajo","dBA","26","36"]
["","","","Alto","dBA","38","44"]
["Accesorios estándar","Manual de instalación","","","","1","1"]
["","Manual de uso","","","","1","1"]
["","Mando a distancia sin cable","","","","1","1"]
["","Pilas secas AAA","","","","2","2"]
["","Soporte del mando a distancia","","","","1","1"]
["","Tubo flexible de drenaje","","","","1","1"]
["","Placa de instalación","","","","1","1"]
["","Aislamiento térmico (tubo de aislamiento térmico)","","","","1","1"]
["","Filtro desodorizante de apatito de titanio","","","","2","2"]
["Sistemas de control","Infrared remote control","","","","ARC466A2","ARC466A2"]
["Conexiones de tubería","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","D.E.","mm","9.50","12.7"]
["","Drain","","","","18","18"]
["Consumo","Refrigeración","","Nom.","kW","0.019 (1), 0.019 (2), 0.019 (3)","0.032 (1), 0.032 (2), 0.032 (3)"]
["","Calefacción","","Nom.","kW","0.022 (1), 0.022 (2), 0.022 (3)","0.035 (1), 0.035 (2), 0.035 (3)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","54","56"]
["","Calefacción","","","dBA","55","58"]
["Dimensiones","Unidad","","Anchura","mm","950","950"]
["","","","Profundidad","mm","215","215"]
["","","","Altura","mm","600","600"]
["Carcasa","Color","","","","Blanco fresco (6.5Y 9.5/0.5)","Blanco fresco (6.5Y 9.5/0.5)"]
["Peso","Unidad","","","kg","22.0","22.0"]
["Power supply","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Nombre","","","","V1","V1"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Cuando se conecta a una unidad exterior múltiple, el nivel de presión sonora en funcionamiento silencioso y el calor radiante es igual a los valores anteriores + 1dB.","(4) - Cuando se conecta a una unidad exterior múltiple, el nivel de presión sonora en funcionamiento silencioso y el calor radiante es igual a los valores anteriores + 1dB."]
["Consumo","Refrigeración","","Nom.","kW","","","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)"]
["","Calefacción","","Nom.","kW","","","0.024 (1) (2) (3), 0.024 (1) (2) (3), 0.024 (1) (2) (3)"]
["Carcasa","Color","","","","","","Blanco fresco (6.5Y 9.5/0.5)"]
["Dimensiones","Unidad","","Altura","mm","","","600"]
["","","","Anchura","mm","","","950"]
["","","","Profundidad","mm","","","215"]
["Peso","Unidad","","","kg","","","22.0"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","","9.1"]
["","","","Medio","m³/min","","","7.2"]
["","","","Bajo","m³/min","","","5.3"]
["","","","Funcionamiento silencioso","m³/min","","","4.5"]
["","","Calefacción","Alto","m³/min","","","10.2"]
["","","","Medio","m³/min","","","8.0"]
["","","","Bajo","m³/min","","","5.8"]
["","","","Funcionamiento silencioso","m³/min","","","5.0"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","55"]
["","Calefacción","","","dBA","","","56"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","39"]
["","","","Medio","dBA","","","33"]
["","","","Bajo","dBA","","","27"]
["","","","Funcionamiento silencioso","dBA","","","24"]
["","Calefacción","","Alto","dBA","","","40"]
["","","","Medio","dBA","","","33"]
["","","","Bajo","dBA","","","27"]
["","","","Funcionamiento silencioso","dBA","","","23"]
["Conexiones de tubería","Líquido","","D.E.","mm","","","6.35"]
["","Gas","","D.E.","mm","","","9.50"]
["","Drenaje","","","","","","18"]
["Sistemas de control","Infrared remote control","","","","","","ARC466A2"]
["Accesorios estándar","Installation manual","","","","","","1"]
["","Wireless remote control","","","","","","1"]
["","Installation plate","","","","","","1"]
["","Thermal insulation (thermal insulation tube)","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","Operation manual","","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","","2"]
["","Drain hose","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Alimentación eléctrica","Nombre","","","","","","V1"]
["","Fase","","","","","","1~"]
["","Alimentación eléctrica-=-Frecuencia","","Frecuencia","","","","50"]
["","Alimentación eléctrica-=-Tensión","","Tensión","","","","220-240"]