{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":11,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F"]
[]
[]
[]
[]
["","","","","","FVXM25FV1B9","FVXM25FV1B","FVXM50FV1B9","FVXM50FV1B","FVXM35FV1B","FVXM35FV1B9"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","38","38","45","45","39","39"]
["","","","Medio","dBA","32","32","40","40","33","33"]
["","","","Funcionamiento silencioso","dBA","23","23","32","32","24","24"]
["","","","Bajo","dBA","26","26","36","36","27","27"]
["","Refrigeración","","Medio","dBA","32","32","40","40","33","33"]
["","","","Funcionamiento silencioso","dBA","23","23","32","32","24","24"]
["","","","Bajo","dBA","26","26","36","36","27","27"]
["","","","Alto","dBA","38","38","44","44","39","39"]
["Accesorios estándar","Manual de instalación","","","","1","1","1","1","1","1"]
["","Manual de uso","","","","1","1","1","1","1","1"]
["","Mando a distancia sin cable","","","","1","1","1","1","1","1"]
["","Pilas secas AAA","","","","2","2","2","2","2","2"]
["","Soporte del mando a distancia","","","","1","1","1","1","1","1"]
["","Tubo flexible de drenaje","","","","1","1","1","1","1","1"]
["","Lámina aislante","","","","2","2","2","2","2","2"]
["","Filtro desodorizante de apatito de titanio","","","","2","2","2","2","2","2"]
["","Placa de instalación","","","","1","1","1","1","1","1"]
["Sistemas de control","Infrared remote control","","","","ARC452A1","ARC452A1","ARC452A1","ARC452A1","ARC452A1","ARC452A1"]
["Conexiones de tubería","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5","12.7","12.7","9.5","9.5"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Consumo","Refrigeración","","Nom.","kW","0.015 (1)","0.015 (1)","0.027 (1)","0.027 (1)","0.015 (1)","0.015 (1)"]
["","Calefacción","","Nom.","kW","0.017 (1)","0.017 (1)","0.034 (1)","0.034 (1)","0.017 (1)","0.017 (1)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","52","52","57","57","52","52"]
["","Calefacción","","","dBA","52","52","58","58","52","52"]
["Dimensiones","Unidad","","Anchura","mm","700","700","700","700","700","700"]
["","","","Profundidad","mm","210","210","210","210","210","210"]
["","","","Altura","mm","600","600","600","600","600","600"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","","kg","14","14","14","14","14","14"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","8.8","8.8","11.8","11.8","9.4","9.4"]
["","","","Bajo","m³/min","5.0","5.0","8.5","8.5","5.2","5.2"]
["","","","Medio","m³/min","6.9","6.9","10.1","10.1","7.3","7.3"]
["","","","Funcionamiento silencioso","m³/min","4.4","4.4","7.1","7.1","4.7","4.7"]
["","","Refrigeración","Bajo","m³/min","4.8","4.8","7.8","7.8","4.9","4.9"]
["","","","Medio","m³/min","6.5","6.5","8.9","8.9","6.7","6.7"]
["","","","Alto","m³/min","8.2","8.2","10.1","10.1","8.5","8.5"]
["","","","Funcionamiento silencioso","m³/min","4.1","4.1","6.6","6.6","4.5","4.5"]
["Power supply","Fase","","","","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50"]
["","Tensión","","","V","220-230-240","220-230-240","220-230-240","220-230-240","220-230-240","220-230-240"]
["Notas","","","","","(1) - 50 Hz, 220-230-240 V","(1) - 50 Hz, 220-230-240 V","(1) - 50 Hz, 220-230-240 V","(1) - 50 Hz, 220-230-240 V","(1) - 50 Hz, 220-230-240 V","(1) - 50 Hz, 220-230-240 V"]
["","","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]