{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":12,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAA-A"]
[]
[]
[]
[]
["","","","","","FXAA25AUV1B","FXAA63AUV1B","FXAA40AUV1B","FXAA50AUV1B","FXAA20AUV1B","FXAA32AUV1B","FXAA15AUV1B (Archived)"]
["Conexiones de tubería","Líquido","","Tipo","","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada"]
["Conexiones de tubería","Gas","","D.E.","mm","9.52","12.70","12.70","12.70","9.52","9.52","9.52"]
["Conexiones de tubería","Líquido","","D.E.","mm","6","6","6","6","6","6"]
["","Gas","","Tipo","","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada"]
["Consumo (50 Hz)","Refrigeración","","A velocidad alta del ventilador","kW","0.028","0.050","0.025","0.033","0.019","0.030","0.017"]
["Nivel de presión sonora","Calefacción","","A velocidad baja del ventilador","dBA","28.5","38.5","33.5","35.5","28.5","28.5","28.5"]
["Conexiones de tubería","Drenaje","","","","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)"]
["Filtro de aire","Tipo","","","","Extraíble / Lavable","Extraíble / Lavable","Extraíble / Lavable","Extraíble / Lavable","Extraíble / Lavable","Extraíble / Lavable","Extraíble / Lavable"]
["Ventilador","Caudal de aire (50 Hz)","Refrigeración","A velocidad baja del ventilador","m³/min","6.5","12.9","9.8","10.9","6.5","6.5","6.5"]
["","","","A velocidad alta del ventilador","m³/min","8.3","18.2","12.2","14.2","7.9","9.4","7.1"]
["Consumo (50 Hz)","Calefacción","","A velocidad alta del ventilador","kW","0.034","0.060","0.030","0.039","0.029","0.035","0.025"]
["Nivel de presión sonora","Refrigeración","","A velocidad baja del ventilador","dBA","28.5","38.5","33.5","35.5","28.5","28.5","28.5"]
["","Calefacción","","A velocidad alta del ventilador","dBA","36.0","47.0","38.0","42.0","34.0","38.5","33.0"]
["","","","A velocidad media del ventilador","dBA","32.5","43.0","36.0","39.0","31.5","33.5","31.0"]
["","","","A velocidad media del ventilador","dBA","32.0","42.5","35.5","38.5","31.0","33.0","30.5"]
["","","","A velocidad alta del ventilador","dBA","35.0","46.5","37.0","41.0","33.0","37.5","32.0"]
["Nivel de potencia sonora","Refrigeración","","A velocidad alta del ventilador","dBA","53.0","63.0","55.0","58.0","52.0","55.0","51.0"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","","kg","12","15","15","15","12","12","12"]
["Dimensiones","Unidad","","Profundidad","mm","266","269","269","269","266","266","266"]
["","","","Anchura","mm","795","1050","1050","1050","795","795"]
["","","","Altura","mm","290","290","290","290","290","290","290"]
["Capacidad de calefacción","Capacidad total","","A velocidad alta del ventilador","kW","3.2","8.0","5.0","6.3","2.5","4.0","1.9"]
["Capacidad de refrigeración","Capacidad total","","A velocidad alta del ventilador","kW","2.8","7.1","4.5","5.6","2.2","3.6","1.7"]
["Refrigerante","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Accesorios estándar","Installation plate","","","","1","1","1","1","1","1","Installation plate"]
["","General safety precautions","","","","1","1","1","1","1","1","General safety precautions"]
["","Wire clamp material","","","","4","4","4","4","4","4","Wire clamp material"]
["","Heat insulating tape","","","","1","1","1","1","1","1","Heat insulating tape"]
["","Installation and operation manual","","","","1","1","1","1","1","1","Installation and operation manual"]
["","Installation pattern","","","","1","1","1","1","1","1","Installation pattern"]
["","Screw bag","","","","1","1","1","1","1","1","Screw bag"]
["Corriente (50 Hz)","Corriente (50 Hz)-=-Amperios máximos del fusible (MFA)-=-A","","","A","6","6","6","6","6","6","6"]
["Alimentación eléctrica","Nombre","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Alimentación eléctrica-=-Frecuencia","","Frecuencia","","50","50","50","50","50","50","50"]
["","Alimentación eléctrica-=-Tensión","","Tensión","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Dimensiones","Dimensiones-=-Unidad-=-Anchura","","","mm","","","","","","","795"]
["Conexiones de tubería","Conexiones de tubería-=-Líquido-=-D.E.","","","mm","","","","","","","6"]