{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","FXFA100A2VEB","FXFA125A2VEB"]
["Dimensiones","Altura","","mm","246","288"]
["","Dimensiones-=-Unidad-=-Profundidad","","mm","840","840"]
["Unidad","kg","","","24","26"]
["Capacidad de refrigeración","Cooling capacity-=-Total capacity-=-At high fan speed","","kW","11.20","14.00"]
["Capacidad de calefacción","Heating capacity-=-Total capacity-=-At high fan speed","","kW","12.50","16.00"]
["Ventilador","Caudal de aire (50 Hz)","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At high fan speed","m³/min","28.8","33.0"]
["","","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At low fan speed","m³/min","13.8","20.6"]
["Consumo (50 Hz)","Power input - 50Hz-=-Cooling-=-At high fan speed","","kW","0.078","0.103"]
["","Power input - 50Hz-=-Heating-=-At high fan speed","","kW","0.078","0.103"]
["Nivel de presión sonora","Sound pressure level-=-Cooling-=-At high fan speed","","dBA","43.0","45.0"]
["","Sound pressure level-=-Cooling-=-At medium fan speed","","dBA","37.0","41.0"]
["","Sound pressure level-=-Heating-=-At high fan speed","","dBA","43.0","45.0"]
["","Sound pressure level-=-Heating-=-At medium fan speed","","dBA","37.0","41.0"]
["","Sound pressure level-=-Cooling-=-At low fan speed","","dBA","30.0","36.0"]
["Nivel de potencia sonora","Sound power level-=-Cooling-=-At high fan speed","","dBA","60.0","61.0"]
["Panel decorativo","Panel decorativo-=-Dimensiones-=-Anchura","","mm","950","950"]
["Nivel de presión sonora","Sound pressure level-=-Heating-=-At low fan speed","","dBA","30.0","36.0"]
["Panel decorativo","Panel decorativo-=-Dimensiones-=-Altura","","mm","65","65"]
["Panel decorativo 2-=-Peso","kg","","","10.3","10.3"]
["Panel decorativo","Panel decorativo-=-Dimensiones-=-Profundidad","","mm","950","950"]
["Panel decorativo-=-Peso","kg","","","5.5","5.5"]
["Panel decorativo 2","Panel decorativo 2-=-Dimensiones-=-Altura","","mm","148","148"]
["","Panel decorativo 2-=-Dimensiones-=-Anchura","","mm","950","950"]
["","Panel decorativo 2-=-Dimensiones-=-Profundidad","","mm","950","950"]
["Conexiones de tubería","Piping connections-=-Gas-=-OD","","mm","15.90","15.90"]
["Panel decorativo 3","Panel decorativo 3-=-Dimensiones-=-Anchura","","mm","950","950"]
["","Panel decorativo 3-=-Dimensiones-=-Altura","","mm","106","106"]
["","Panel decorativo 3-=-Dimensiones-=-Profundidad","","mm","950","950"]
["Panel decorativo 3-=-Peso","kg","","","6.5","6.5"]
["Accesorios estándar","Washer for hanger bracket","","","8","8"]
["","Wire clamp material","","","7","7"]
["","Clamp for drain hose","","","1","1"]
["","Clamps","","","1","1"]
["","Drain hose","","","1","1"]
["","Installation and operation manual","","","1","1"]
["","Installation guide","","","1","1"]
["","Insulation for fitting","","","2","2"]
["","Screws","","","4","4"]
["","Sealing pads","","","1","1"]
["Alimentación eléctrica","Alimentación eléctrica-=-Tensión","","","220-240/220","220-240/220"]
["","Alimentación eléctrica-=-Frecuencia","","","50/60","50/60"]
["Corriente (50 Hz)-=-Amperios máximos del fusible (MFA)","A","","","6","6"]
["Name","","","","1","1"]