{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Carcasa","Color","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","500"]
["","Dimensiones-=-Unidad-=-Anchura","","","mm","270"]
["","","","Profundidad","mm","270"]
["Peso","Unidad","","","kg","6.8"]
["Operación de purificación de aire","Consumo","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","B","kW","0.010"]
["","","","Funcionamiento silencioso","kW","0.008"]
["Nivel de presión sonora","Operación de purificación de aire","","Turbo","dBA","53"]
["","","","Media","dBA","39"]
["","","","Bajo","dBA","29"]
["","","","Funcionamiento silencioso","dBA","19"]
["Ventilador","Caudal de aire","Operación de purificación de aire","Turbo","m³/h","330"]
["","","","Medio","m³/h","192"]
["","","","Bajo","m³/h","120"]
["","","","Funcionamiento silencioso","m³/h","66"]
["Dispositivos de seguridad","Elemento","","01","","Interruptor de seguridad (el funcionamiento se detiene cando la cubierta de la unidad Streamer está abierta)"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50/60"]
["","Tensión","","","VCA","220-240/220-230"]
["Corriente de funcionamiento","Operación de purificación de aire","","Turbo","A","0.32"]
["","","","Media","A","0.14"]
["","","","Baja","A","0.10"]
["","","","Funcionamiento silencioso","A","0.08"]