{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Carcasa","Color","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","700 (1)"]
["","Dimensiones-=-Unidad-=-Anchura","","","mm","270"]
["","","","Profundidad","mm","270 (4)"]
["Peso","Unidad","","","kg","9.5"]
["Operación de purificación de aire","Consumo","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","B","kW","0.010"]
["","","","Funcionamiento silencioso","kW","0.007"]
["Función de humidificación","Consumo","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","B","kW","0.014"]
["","","","Funcionamiento silencioso","kW","0.011"]
["","Capacidad del depósito de agua","","","l","2.7"]
["Nivel de presión sonora","Operación de purificación de aire","","Turbo","dBA","53.0"]
["","","","Media","dBA","39.0"]
["","","","Bajo","dBA","29.0"]
["","","","Funcionamiento silencioso","dBA","19.0"]
["","Función de humidificación","","Turbo","dBA","53.0"]
["","","","Medio","dBA","39.0"]
["","","","Bajo","dBA","33.0"]
["","","","Funcionamiento silencioso","dBA","25.0"]
["Ventilador","Caudal de aire","Operación de purificación de aire","Turbo","m³/h","330"]
["","","","Medio","m³/h","192"]
["","","","Bajo","m³/h","120"]
["","","","Funcionamiento silencioso","m³/h","54"]
["","","Función de humidificación","Turbo","m³/h","330"]
["","","","Medio","m³/h","192"]
["","","","Bajo","m³/h","144"]
["","","","Funcionamiento silencioso","m³/h","102"]
["Accesorios estándar","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50/60"]
["","Tensión","","","VCA","220-240/220-230"]
["Corriente de funcionamiento","Operación de purificación de aire","","Turbo","A","0.50"]
["","","","Media","A","0.19"]
["","","","Baja","A","0.12"]
["","","","Funcionamiento silencioso","A","0.09"]
["","Función de humidificación","","Turbo","A","0.50"]
["","","","Media","A","0.20"]
["","","","Baja","A","0.15"]
["","","","Funcionamiento silencioso","A","0.13"]
["Notas","","","","","(1) - Solo trifásico"]
["","","","","","(2) - Otras funciones: Función de reinicio automático."]
["","","","","","(3) - Safety valve"]
["","","","","","(4) - Prueba con Ta BS/BH 14°C/13°C. Conforme a EN 16147."]