{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","39","40","41"]
["","","Medio","dBA","34","34","35"]
["","","Funcionamiento silencioso","dBA","25","25","26"]
["","","Bajo","dBA","28","28","29"]
["","Refrigeración","Medio","dBA","33","33","34"]
["","","Funcionamiento silencioso","dBA","22","22","23"]
["","","Bajo","dBA","25","26","27"]
["","","Alto","dBA","39","40","41"]
["Accesorios estándar","Manual de instalación","","","1","1","1"]
["","Manual de uso","","","1","1","1"]
["","Mando a distancia sin cable","","","1","1","1"]
["","Pilas secas AAA","","","2","2","2"]
["","Soporte del mando a distancia","","","1","1","1"]
["","Placa de montaje","","","1","1","1"]
["","Filtro desodorizante de apatito de titanio","","","2","2","2"]
["","Tornillos de fijación de la unidad interior","","","2","2","2"]
["Sistemas de control","Infrared remote control","","","ARC433A87","ARC433A87","ARC433A87"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.50","9.50","9.50"]
["","Drain","","","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.030","0.030","0.030"]
["","Calefacción","Nom.","kW","0.040","0.040","0.040"]
["Nivel de potencia sonora","Refrigeración","","dBA","55","55","58"]
["","Calefacción","","dBA","55","55","58"]
["Dimensiones","Unidad","Anchura","mm","770","770","770"]
["","","Profundidad","mm","283","283","283"]
["","","Altura","mm","198","198","198"]
["Carcasa","Color","","","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","7.00","7.00","7.00"]
["Power supply","Fase","","","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50"]
["","Nombre","","","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240"]